SHIP: FEDERATION: STARSHIP: CLASS DETAILS:

Class: Nebula (Side View)
Type: Explorer

DISPLACEMENT
Light: 2,775,000 MT
Standard: 3,309,000 MT
Full: 3,750,000 MT
Cargo Capacity: 735,000 MT

DIMENSIONS
Length: 442.23 m
Beam: 318.11 m
Draught: 130.43 m
Number of Decks: 33

PROPULSION
Warp Drive: M/ARA Mark I feeding 2 GN-3 Mod 2 Warp Drive Nacelles
Warp Engine Fuel: Cold Deuterium (matter) / Anti-Hydrogen (antimatter)
Impulse Drive: 2 LMP Fusion Reaction Impulse Units
Impulse Engine Fuel: Slush Deuterium
Fuel Replenishment: Bussard Scoop
Reaction Control System: Fusion Thrust Units

VELOCITY
Normal Cruising Speed: Warp 6
Max Cruising Speed: Warp 9

ACCELERATION
Rest-Onset Critical Momentum: 5.39 sec
Onset Critical Momentum-Warp Engage: .11 sec
Warp 1-Warp 3: .14 sec
Warp 3-Warp 6: .11 sec
Warp 6-Warp 9: .19 Sec

DURATION
Expected Lifetime: Estimated 100 Years
Number of Maintaince/Upgrade Layovers: 200
Time Between Resupply: 5 Years
Time Between Refit: 20 Years

COMPLEMENT
Officer Crew: 173
Enlisted Crew: 577
Civilians/Families: none
Evacuation Capacity: 9,800

EMBARKED CRAFT
Total: 20

NAVIGATION
System: "Cosmosis" Warp Celestial Guidance

COMPUTERS
Type: FTL Mk I
Crew Interface Software: LCARS 2.3
Data Transfer Rate: 4600 Kiloquads/Second
Number of Dedicated Modules: 2048
Storage Capacity/Module: 630,000 Kiloquads

SENSORS
High Resolution Long Range Max Effective Range: 5 ly
Medium to Low Resolution Effective Range: 17 ly

COMMUNICATIONS
Intraship Transmissions: Voice & Data
Personnel Communicator Range: 500 km
Ship to Ground Range: 38,000 - 60,000 km
Communications Speed: 18.5 Kiloquads/Second
Subspace Speed: 9.9997 Warp

PHASERS
Ship: 8 Type X Phasers: 4.9 MW

PHOTON TORPEDOES
Tubes: 2 Mk 10 Mod 5 Direct
Max Torpedo Simultaneous Spread: 10

DEFENSE
Shields: "Hercules" Primary Force Field and Deflector Control System
Fire Control: "Monitor V" Fire Control System

TRANSPORTERS
Personnel Transporters: 4
Emergency Transporters: 4
Cargo Transporters: 6