SHIP: FEDERATION: SPACE STATION: CLASS DETAILS:

Class: K (Side View)

DISPLACEMENT
Light: 360,000 MT
Standard: 395,000 MT
Full: 430,000 MT
Cargo Capacity: 10,000 MT

DIMENSIONS
Primary Complex Maximum Diameter: 104.796 m
Primary Complex Maximum Depth: 97.128 m
Secondary Complex Maximum Diameter: 75.146 m
Secondary Complex Maximum Depth: 55.72 m
Central Complex Maximum Diameter: 37.318 m
Central Complex Maximum Depth: 19.426 m
Docking Port Maximum Diameter: 47.797 m
Docking Port Maximum Depth: 18.25 m
Support Pylon Length Overall: 104.796 m
Support Pylon Maximum Diameter: 18.576 m
Draught: 160.517 m
Number of Decks: 35

POWER SYSTEM
Primary Power System: 1 Fusion Reactor
Station Keeping Thrusters: SC44B Chemical Combustion Precise Control Package; Magnafield Gyro

DURATION
Expected Lifetime: Estimated 100 Years
Time Between Resupply: 2 Years
Time Between Refit: 5 Years

COMPLEMENT
Officer Crew: 86
Enlisted Crew: 712
Civilian/Families: 0
Evacuation Capacity: 1000

EMBARKED CRAFT
Work Bees: 6
Shuttles: 2
Resue Pod: 1
Repair Craft: 2

COMPUTERS
Type: "Daystrom" Duotronic II

SENSORS
High Resolution Long-Range Scan Maximum Range: 1.9 ly
Medium to Low Resolution Range: 3.1 ly

COMMUNICATIONS
Intrastation Transmissions: Voice & Data
Personnel Communicator Range: 300 km
Ship to Ground Range: 33,000 - 47,000 km
Communications Speed: 18.5 Kiloquads/Second
Subspace Speed: 9.9997 Warp

DEFENSE
Shields: Hycor Modular Adaptive Force Field and Deflector System

TRANSPORTERS
Personnel Transporters: 6
Emergency Transporters: 5
Cargo Transporters: 2