SHIP: FEDERATION: STARSHIP: CLASS DETAILS:

Class: Galaxy (Top View)
Type: Explorer

DISPLACEMENT
Light: 4,125,000 MT
Standard: 4,500,000 MT
Full: 4,850,000 MT
Cargo Capacity: 875,000 MT

DIMENSIONS
Length: 642.51 m
Beam: 463.73 m
Draught: 195.26 m
Number of Decks: 42

PROPULSION
Warp Drive: M/ARA Mark I feeding 2 GN-1 Mod 1 Warp Drive Nacelles
Warp Engine Fuel: Cold Deuterium (matter) / Anti-Hydrogen (antimatter)
Impulse Drive: 3 LMP Fusion Reaction Impulse Units
Impulse Engine Fuel: Slush Deuterium
Fuel Replenishment: Bussard Scoop
Reaction Control System: Fusion Thrust Units

VELOCITY
Normal Cruising Speed: Warp 6
Max Cruising Speed: Warp 9.2

ACCELERATION
Rest-Onset Critical Momentum: 5.61 sec
Onset Critical Momentum-Warp Engage: .13 sec
Warp 1-Warp 3: .17 sec
Warp 3-Warp 6: .15 sec
Warp 6-Warp 9: .23 Sec

DURATION
Expected Lifetime: Estimated 100 Years
Number of Maintaince/Upgrade Layovers: 200
Time Between Resupply: 5 Years
Time Between Refit: 20 Years

COMPLEMENT
Officer Crew: 185
Enlisted Crew: 725
Civilians/Families: 250+
Evacuation Capacity: 15,000

EMBARKED CRAFT
Total: 40

NAVIGATION
System: "Cosmosis" Warp Celestial Guidance

COMPUTERS
Type: FTL Mk I
Crew Interface Software: LCARS 2.3
Data Transfer Rate: 4600 Kiloquads/Second
Number of Dedicated Modules: 2048
Storage Capacity/Module: 630,000 Kiloquads

SENSORS
High Resolution Long Range Max Effective Range: 5 ly
Medium to Low Resolution Effective Range: 17 ly

COMMUNICATIONS
Intraship Transmissions: Voice & Data
Personnel Communicator Range: 500 km
Ship to Ground Range: 38,000 - 60,000 km
Communications Speed: 18.5 Kiloquads/Second
Subspace Speed: 9.9997 Warp

PHASERS
Ship: 11 Type X Phasers: 5.1 MW
Personal: Type I, II & III Phasers: 0.01MW

PHOTON TORPEDOES
Tubes: 3 Mk 10 Mod 5 Direct
Max Torpedo Simultaneous Spread: 10

DEFENSE
Shields: "Hercules" Primary Force Field and Deflector Control System
Fire Control: "Monitor V" Fire Control System

TRANSPORTERS
Personnel Transporters: 6
Emergency Transporters: 6
Cargo Transporters: 8