SHIP: FEDERATION: SHUTTLE: CLASS DETAILS:

Class: Atai (Side View)
Type: Class 5
Model: MK-XId
Mission Type: Heavy Long-Range Sublight Shuttle

DISPLACEMENT
Light: 8.73 MT
Standard: 9.49 MT
Full: 10.91 MT

DIMENSIONS
Length: 18.7 m
Beam: 11.14 m
Draught: 4.44 m

POWER PLANT
Engines: 1 DP3/5-Q Impulse Drive Unit
Reaction Control System: 8 "Artemis" Pulsed Laser RCS Thrusters 

PERFORMANCE
Maximum Delta-v 17,250 m/sec

COMPLEMENT
Crew: 4 (Pilot, Co-Pilot, Navigator, and Systems Manager)
Passengers: 14 (Standard); 4 (Diplomatic); 24 (Emergency)

ARMAMENT
1 bank of 2 each - SAR-2 Independent Twin Mount; 2 banks - SIR-1 Single Mount


FEDERATION WARP SLED (Vulcan)

Class: Tai
Type: Class 6
Model: MK-XV
Mission Type: Long-range Warp drive shuttle attachment

DISPLACEMENT
Light: 74.73 MT
Standard: 81.23 MT
Full: 93.41 MT

DIMENSIONS
Length: 48.7 m
Beam: 26.73 m
Draught: 8.72 m

POWER PLANT
Engines: Linear Intermix M/ARA feeding 2 IPE25E/4-IU Dilithium-Energized Antimatter Linear Warp Drive Micro-Nacelles; 2 SW25/2-10S Impulse Drive Units
Reaction Control System: 4 "Artemis" Pulsed Laser RCS Thrusters 

PERFORMANCE
Warp 4 for 96 hours; Warp 4.5 for 48 hours; Warp 4.78 for 36 hours*
* Following old Warp standards.

ARMAMENT
None
















































